IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2016-07-07T11:42:15"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.13.0.0"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "batyg" of Organization (no name given)
  Owner history of Person "batyg" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1453219000 (2016-01-19T15:56:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCELECTRICAPPLIANCETYPE "Slim Line Recessed Warm Air Dryer" | object type "Slim Line Recessed Warm Air Dryer" | names: "NBS_DudleyIndustriesLimited_HandDriers_SlimLineRecessedWarmAirDryer:Slim Line Recessed Warm Air Dryer:218871" | material: "NBS_Concept" | property sets: COBie

Types
  IFCELECTRICAPPLIANCETYPE "Slim Line Recessed Warm Air Dryer" | HANDDRYER | 1 occurrence | material: "NBS_Concept" | property sets: NBS_General, NBS_Data, Pset_FurnitureTypeCommon, Pset_DoorWindowGlazingType, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_70_62_37:Hand driers" (IFCTEXT)
    CodePerformance = "CE Marked, BS EN 60335-2-23:2003 + *A1:2008 (Particular Requirements for Appliances for skin and hair Care) and BSEN60335-1:2002 + *A2:2006 (incorporating *A1,*A11,*A12, *A13 (Safety of Household and similar electrical appliances), EN55014-1: 2006 + A1: 2009*, EN55014-2: 1997 + A1: 2001 + A2:2008*, EN61000-3-2: 2006, EN61000-3-3: 2008*, Tests marked * are not covered under SGS UKAS Scope, RoHS, WEEE" (IFCTEXT)
    Color = "Satin stainless steel" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Stylish satin stainless steel warm air dryer" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10" (IFCTEXT)
    Features = "Clean ergonomic design, Suitable for 100mm wall cavities, Durable stainless steel enclosure, Seam welded fabrication, Integral painted metal liner, Available as an individual unit or with Waste Bin and Paper Towel dispenser, 'No' Touch Automatic operation by infrared sensor built into the air outlet, Automatic start/stop, CE Marked, RoHS, WEEE" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@dudleyindustries.com" (IFCTEXT)
    Material = "Brushed stainless steel" (IFCTEXT)
    ModelNumber = "92282SS" (IFCTEXT)
    ModelReference = "Slimline Recessed Warm Air Dryer" (IFCTEXT)
    Name = "HandDriers_SlimLineRecessedWarmAirDryer_DudleyIndustriesLimited" (IFCTEXT)
    NominalHeight = 579. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 382.00000058064 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 382. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "100% Recycleable" (IFCTEXT)
    WarrantyDescription = "Parts & Labour" (IFCTEXT)
    WarrantyDurationLabor = "year" (IFCTEXT)
    WarrantyDurationParts = "year" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "5" (IFCTEXT)
    WarrantyGuarantorParts = "5" (IFCTEXT)
  NBS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_DudleyIndustriesLimited_HandDriers_SlimLineRecessedWarmAirDryer" (IFCTEXT)
    ManufacturerName = "Dudley Industries Limited" (IFCTEXT)
    ManufacturerURL = "www.dudleyindustries.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/zoj5rpu3" (IFCTEXT)
    NBSDescription = "Hand driers" (IFCTEXT)
    NBSNote = "n/a" (IFCTEXT)
    NBSOfficeMasterTag = "n/a" (IFCTEXT)
    NBSReference = "45-35-72/334" (IFCTEXT)
    NBSTypeID = "n/a" (IFCTEXT)
    ProductInformation = "www.dudleyindustries.com/product/slim-line-recessed-warm-air-dryer/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_70_62_37" (IFCTEXT)
    Uniclass2015Title = "Hand driers" (IFCTEXT)
    Uniclass2015Version = "Products v1.4" (IFCTEXT)
    Version = "2" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    AirOutput = "21 m/s" (IFCTEXT)
    BodyColourAndFinish = "Satin stainless steel" (IFCTEXT)
    BodyEnclosure = "304 Stainless steel" (IFCTEXT)
    BodyIngressProtectionMinimum = "IP21" (IFCTEXT)
    EquipmentElectricalPower = "208–240 V AC, 1400–1900 W" (IFCTEXT)
    Form = "Recessed, Wall mounted" (IFCTEXT)
    HandDryingTime = "15-20 s" (IFCTEXT)
    MotorRotationFrequency = "n/a" (IFCTEXT)
    NoiseLevelAtOneMetre = "81.5 dBA" (IFCTEXT)
    Operation = "Automatic. No touch" (IFCTEXT)
    PowerRating = "1400–1900 W" (IFCTEXT)
    Weight = "14.3 kg" (IFCTEXT)
  Pset_FurnitureTypeCommon | properties | on 1 type object
    Description = "Stylish satin stainless steel warm air dryer" (IFCTEXT)
    MainColor = "Satin stainless steel" (IFCTEXT)
    NominalDepth = 116. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 579. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 382.00000058064 (IFCLENGTHMEASURE) [MILLI METRE]
    Style = "Hand Dryer" (IFCTEXT)
  Pset_DoorWindowGlazingType | properties | on 1 type object
    HasProtectiveEarth = TRUE (IFCBOOLEAN)
    IP_Code = "n/a" (IFCTEXT)
    InsulationStandardClass = "n/a" (IFCTEXT)
    NominalFrequencyRange = "n/a" (IFCTEXT)
    NominalVoltage = "n/a" (IFCTEXT)
    PhaseReference = "n/a" (IFCTEXT)